COSHH ASSESSMENT NCS/FM/070 Issue005/Jul09

Ref: COSHH 03

Assessed by: Matt Traynor Position: Managing Director

Date: January 2022



Reviewed by: Matt Traynor Position: Managing Director

Date: January 2022

Issue: 008 Jan 22

Trade name / Supplier: Telephone number:

Contact:

Toxic Corrosive



Product type:

Hydraulic Oil

Irritant



Highly



Flammable



Chemicals and appearances:

Mineral and / or Hydrocarbon

Harmful



Oxidising

|  |  |
| --- | --- |
| Risk associated with use: | Prolonged skin contact can lead to dermatitis and skin cancer. Irritating to skin, eyes and respiratory system |
|  |  |
| Personal Protection: | Wear overalls and rubber gloves. Do not eat, drink or smoke when using |
|  |  |
| Storage: | Store and use from containers designed for use with this product.  Keep containers closed when not in use.  Store and dispense in well ventilated areas - away from heat and sources of ignition |
|  |  |
| Disposal: | Return any unused product to supplier, or plant depot.  Any material contaminated by the product should be designated as special waste, and disposed of through a specialist waste disposal contractor |
|  |  |
| Fire: | Powder, foam halon or Carbon Dioxide extinguishers must be available at storage areas  DO NOT USE WATER  Empty containers represent a fire hazard, do not accumulate, return to supplier |
|  |  |
| Spillage: | Confine and absorb with inert material e.g. sand.  Collect any leaking liquid in containers and clean with detergent. Wear gloves |

Appointment Effect First Aid

Dermatitis, possible skin cancer

Skin

Wash well with plenty of soap and water.

Remove contaminated clothing. Seek medical advice if irritation persisits

Irritation, stinging Flush eyes with copious quantity of water.

Eyes

If irritation persists, seek medical advice

Inhalation Irritation to nose and throat Move to fresh air and rest. If symptoms persist seek medical advice

Irritation, nausea DO NOT INDUCE VOMITING.

Swallowing

Wash mouth out with water and seek medical advice